{"text_format":"1","workbook":"xlsx","n_sheets":10,"sheets":["計算","使用方法","解説","精度","SIM","記号表","test","weep data","%Flood詳細解説","Sheet1"],"not_rendered":{"charts":2,"images":4,"macros":1,"external_links":0,"defined_names":0,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"計算","index":0,"n_rows":31,"n_cols":33,"rows_kept":31,"cut":false,"hidden":false,"merged":[]}
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,22,{"$f":"V1+1","v":23},24,25,26,27,28,29,30,31,32,33]
[null,null,null,null," ",null,null,null,null,null,null,null,null,null,null,null,"no of pass",2,"1pass=1: 2pass=2 : 4pass=3"]
["text(1)"," Vapor Rate       (kg/h)",128874,null,null,null,null,"text1","　AT : cross sectinonal　ａｒｅａ (m2)",null,null,9.6211285624999991,null,null,null,null,"valve type",1,"v1=1 : v4=2"]
["text(2)"," Liquid Rate       (kg/h)",283056,null,null,null,null,"text4","　AD1:　downcomer area (m2)",null,null,1.2236049677870375,null,null,null,null,"active area",1,"自動=1　　：手動=2"]
["text(3)"," Vapor density   (kg/m3)",62.2,"text(16)"," No of valve per tray",504,null,"text5","　AD3 : downcomer area (m2)",null,null,2.4541403283524019,null,null,null,null,"notched weir",2,"有り＝１　：なし＝２"]
["text(4)"," Liuid density    (kg/m3)",431.8,"text(17)"," Valve hole ID (mm)",39,null,"text6","　AD5 : downcomer area (m2)",null,null,0,null,null,null,null,"MX",1,"メカ手動入力=1：データﾍﾞｰｽ使用＝２"]
["text(5)"," Allowable max flood%",82,null," Rtio of light  ",null,null,"text7","　AA : active area　　 (m2)",null,null,4.7197782985735222,null,null,null,null,"計算モード",1,"設計=1：ｼﾐｭﾚｰｼｮﾝ=2"]
["text(6)"," System  factor    (-)",1,"text(18)","  type valve (%)",50,null,"text13","　CAF",null,null,0.41424794406244214]
[null,null,null,null,null,null,null,"text12","　VLOAD",null,null,8.337979914066235]
["text(7)"," Column ID     (mm)",3500,null,null,null,null,"text14","　FLOOD ( %)",null,null,70.798460185913655]
["text(8)"," Tray spacing  (mm)",700,null,null,null,null,"text16","　P.DROP-A (mmH2O)",null,null,68.250528750953734]
["text(9)"," Weir height   (mm)",40,null,null,null,null,"text17","　P.DROP-B (mmH2O)",null,null,64.682626837070103]
["text(10)"," Downcomer  clearance(mm)",90.3,null,null,null,null,"text22","　DC.backup-A (%)",null,null,40.699035179059685]
["text(11)"," Tray thickness (mm)",2,"text(19)"," Notch depth (mm)",0,null,"text23","　DC.backup-B (%)",null,null,39.451001387736412]
[null,null,null,"text(20)","Notch pitch (mm)",0,null,"text2","　Under DC velocity-A (ft/s)",null,null,1.2174263263758331]
[null,null,null,null,null,null,null,"text26","　Under DC velocity-B (ft/s)",null,null,0.9650012496248721]
[null,null,null,null,null,null,null,"text25","  Design Piont  Weep Liuid -A (kg/h)",null,null,3046.1684146123507]
[null,null,null,null,null,null,null,"text18","  Design Piont  Weep Liuid -B (kg/h)",null,null,2496.3057028523253,null,null,null,null,null,null,null,null,"% FLOOD",null,70.798460185913655,18]
[null,null,null,null,null,null,null,"text24","　25% weep vapor load-A (%)",null,null,4.392578125,null,null,null,null,null,null,null,null,"undew downcomer velocity －１","(ft/s)",0.9650012496248721,{"$f":"X18+1","v":19}]
["text(12)"," DC Width  H1 (mm)",647,null,null,null,null,null,"　25% weep vapor load-B (%) ",null,null,"非収束",null,null,null,null,null,null,null,null,"undew downcomer velocity －２","(ft/s)",1.2174263263758331,{"$f":"X19+1","v":20}]
["text(13)"," DC Width  H3 (mm)",706,null,null,null,null,null,"　Unit referance (%)",null,null,63.01795973997249,null,null,null,null,null,null,null,"計","pess.drop dry-1","inch liq",3.3260911644671545,21]
["text(14)"," DC width  H5 (mm)",0,"text(21)","Active area (m2)   ",null,null,null," Mini. Vaopr Load  (kg/h)",null,null,30039.15207982521,null,null,null,null,null,null,null,"算","pess.drop dry-2","inch liq",3.3260911644671545,22]
["text(15)"," Flow pass length (mm)",750,null,"手動計算時に入力",0,null,null," Max. Vaopr Load  (kg/h)",null,null,165297.05945164792,null,null,null,null,null,null,null,"結","pess.drop over weir-1","inch liq",2.2668423486927125,23]
[null,null,null,null,null,null,null,null," Min.  Liquid Load  (kg/h)",null,null,36992.09313578486,null,null,null,null,null,null,null,"果","pess.drop over weir-2","inch liq",1.9415329941610837,24]
[null,null,null,null,null,null,null,null," Max. Liquid Load  (kg/h)",null,null,288303.59540239314,null,null,null,null,null,null,null,null,"pess.drop tray-1","mmH2O",68.250528750953734,25]
[null,null,null,null,null,null,null,null,"  注）   -A , -B は偶数、奇数段を示す",null,null,null,null,null,null,null,null,null,null,null,"pess.drop tray-2","mmH2O",64.682626837070103,26]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DC backup -1","(%)",40.699035179059685,27]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"DC backup -2","(%)",39.451001387736412,28]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"unit referance","(%)",63.01795973997249,29]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"25% weep vapor load-1","(%)",4.392578125,{"$f":"X29+1","v":30}]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"25% weep vapor load-2","(%)","非収束",31]

{"sheet":"使用方法","index":1,"n_rows":48,"n_cols":2,"rows_kept":48,"cut":false,"hidden":false,"merged":[]}
["使い方"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
["シートの説明"]
["シート”解説”","トレーの構造、計算時の制約事項などが解説に記載されてます。 最初に読んで下さい。"]
[]
["シート”精度”","エンジニアリング会社の計算値と本計算ソフトを使用した場合の計算値を C-XXXXについて比較してあります。"]
[null,"ほぼ同等な計算結果となっています。 ないのは ”ギャランティー” です。"]
[]
["シート”記号表”","Module マクロを見聞するときに役立つ記号表を記載しました。"]
[]
[]
["使用方法"]
["データの入力","ピンクセルは、手動入力します。 Vapor/ Liquid Rate はPro-Ⅱ 等の蒸留シミュレーター の計算結果を用いる。"]
[null,"青のセルは、メカニカルデータで、手動入力とシート”DATA”からの転送がどちらも可能。"]
[null,"Allowable Max Flood% 、System Factor は解説を参照。"]
[]
["トレーメカデータ","水色セルに入力する。 "]
[]
["計算の実行","全てのデータを入力したら 計算実行 ボタンで実行できます。"]
[]
["計算結果","計算結果が 緑のセルに表示されます。"]

{"sheet":"解説","index":2,"n_rows":197,"n_cols":36,"rows_kept":197,"cut":false,"hidden":false,"merged":[]}
[]
[]
[]
["はじめに"]
[null,"本計算シートは、30年以上前の Glitsch社の”BALLAST TRAY DESIGN MANUAL（BULLETIN#4900）”に基づき作成されています。"]
[null,"2013年にMANUAL 第6版が開示されているが、変更点の確認はしていません。"]
[null,"25%Weeping や Notch Weir の計算は、推定方法による計算なので参考値程度に扱うこと。"]
[null,"メーカーの計算値と精度比較は行っているが、あくまでユーザーの責任で計算結果を判断されたい。"]
[null,"この計算シートは、マクロを使用しているので、マクロを有効で使用して下さい。"]
[null,"マクロ（Module1）には、予期せぬ変更を防ぐためパスワードが設定されています。"]
[]
["用途"]
[null,"この計算シートでは、塔径、トレースペースなどの設定されたデータで、どれだけの気液を処理できるかを計算するものです。"]
[null,"プロダクトの性状は、別のプロセスシミュレーターで計算して下さい。"]
[]
["用語解説"]
[]
["tray load"]
[null,"Vapor rate  trayに入ってくるvaporの量  (kg/h)"]
[null,"liquid rate  trayを出て行くliquidの量 (kg/h)"]
[null,"vapor density  trayに入るvaporの密度 (kg/m3)"]
[null,"liquiddensity  trayを出て行くliquidの密度(kg/m3)"]
[null,"上記の値は､ﾌﾟﾛｾｽｼﾐｭﾚｰﾀｰ又は､trayのﾃﾞｰﾀｼｰﾄにより求める。"]
[null,"Vaporrate、Liquidrateをtowerへの供給量（ﾌｨｰﾄﾞ量）と間違えないこと｡"]
[]
["allowable max flood％"]
[null,"許容される最大のfloog%である。"]
[null,"設計時には、加圧ｻｰﾋﾞｽ（常圧も含む）は 82%"]
[null,"          ﾊﾞｷｭｰﾑｻｰﾋﾞｽは77%"]
[null,"          塔径910mm以下の場合は､ 75% を上限として設計する｡"]
[null,"          （ ADIP液の場合60～ 70% が指定されている。）"]
[null,"towerへのfeed、reflux流量などが安定していれば実際は､82%以上の処理は､可能で"]
[null,"あるが個別にﾕｰｻﾞｰの責任でトライすべき問題である｡"]
[]
["system factor"]
[null,"処理する流体によってfoam（泡立ち）の傾向が異なる。これを補正するのが"]
[null,"system factor（foam factorという呼び方もある）である。以下の値を標準値"]
[null,"として使用する｡"]
[null,"泡立ちしない流体・通常の流体      1.00"]
[null,"fluorine   ex. BF3,freonなど         0.90"]
[null,"中程度のﾌｫｰﾐﾝｸﾞ流体  oil absorber,amine and glycolのregeneratorなど 0.85"]
[null,"ﾌｫｰﾐﾝｸﾞ流体     amine and glycolのabsorbersなど    0.73"]
[null,"                     （ ADIP液の場合0.71が指定されている。）"]
[null,"ひどいﾌｫｰﾐﾝｸﾞ流体       ＭＥＫなど         0.60"]
[null,"連続的にﾌｫｰﾐﾝｸﾞ傾向の流体        caustic regenerator    0.3 ～0.6"]
[]
[" VALVEのﾀｲﾌﾟ"]
[null,"V-1 ﾀｲﾌﾟ"]
[null,"最も一般的に使用されるﾀｲﾌﾟである｡何も指定しなければ、V1を使用する｡"]
[null,"V-4 ﾀｲﾌﾟ"]
[null,"V4 ﾄﾚｰのデッキがﾍﾞﾝﾁｭﾘｰになっていて、ﾊﾞｷｭｰﾑｻｰﾋﾞｽやﾄﾚｰの圧力損失を特に少なくする指定がある時使用する｡"]
[null,"valve hole （ ﾊﾞﾙﾌﾞの取り付けられている穴の内径 ）は39mmである。"]
[null,"Ｈ記号 (  V-1H  V-4H  )"]
[null,"V-1、V-2のユニットに重りを付けて重くしたﾕﾆｯﾄ。全数の50%以上は使用しない｡"]
[]
["Active area"]
[null,"通常はｔｏｗｅｒの断面積からﾀﾞｳﾝｶﾏｰの面積を引いたものがａｃｔｉｖｅareaとなり、自動計算される。"]
[null,"但し､trayにブランキングを実施した場合は､自動計算されたａｃｔｉｖｅareaから ﾌﾞﾗﾝｷﾝｸﾞした面積を引いて ａｃｔｉｖｅ ａｒｅａ とする必要があるので、この場合には､手動入力を選択する｡"]
[]
["downcomer clearance"]
[null,"標準値は､ 40mmである。    （  15mmが下限値  ）"]
[]
["max underｄｏｗｎｃｏｍｅｒvelosity"]
[null,"underＤＣ （downcomer） velosityの上限値は､ 1.24 ft/sである。"]
[null,"計算結果のA,Bは、２ｐａｓｓ ｔｒａｙ のH1 、H3における値である｡"]
[null,"４ｐａｓｓの Ｈ５ における値は､計算していない。"]
[]
["ＤＣ ｂａｃｋｕｐ"]
[null,"ＤＣ(downcomer) ｂａｃｋｕｐ とは、ﾀﾞｳｶﾏｰ内に液が何％溜まっているかを計算している｡"]
[null,"ﾊﾞｯｸｱｯﾌﾟが高くなれば､運転不能となる｡ 許容上限値は､次の値である｡"]
[null,"       Dv ( vaporの密度kg/m3 )          許容上限値（％）"]
[null,"      Dv  ＜  １６       の時              ６０"]
[null,null," １６  ＜＝ Ｄｖ   ＜  ４８ の時         ５０"]
[null,null,"  ４８ ＜＝ Ｄｖ   の時                  ４０"]
[]
["unit referance"]
[null,"ｖａｌｖｅがある瞬間に何％ 開いているかを示す値である。"]
[null,"良好なﾊﾟｰﾌｫｰﾏﾝｽを発揮するためには､最低下記の値が必要である。"]
[null,"       Ｎｏ ｏｆ ｐａｓｓ           minimumｕｎｉｔ ｒｅｆｅｒａｎｃｅ (%)"]
[null,"           １                    ３５以上"]
[null,"           ２                    ５０以上"]
[null,"           ４                    ６５以上"]
[]
["Weeping"]
[null,"蒸留が効果的に行われるには、トレー上で蒸気と液が効果的に接触する必要がある。"]
[null,"downcomer を経由しないで ｖａｌｖｅ hole から液が直接下のトレーに落下する現象が Weeping であり、"]
[null,"Tray上の液の 25%が直接下のトレーに落下する状況が  25%weeping である。 設計時のtray効率は通常 70-80% 程度なので、"]
[null,"25% weeping以上の 液落下になると、トレー蒸留効率が低下し、所定の蒸留性状（品質）が得られなくなる。"]
[null,"一般に、25%weepingに至る Vapor rateは、運転ポイントに比べて相当小さいので、通常運転では問題にならない。"]
[]
[]
["トレーの構造と名称"]
[null,null,null,"1pass tray の構造"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"A",null,"colume ID ",null,null,null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"B",null,"weir height",null,null,null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"C",null,"downcomer width",null,null,null,null,null,"(H1)",null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"D",null,"tray spacing",null,null,null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,"E",null,"downcomer clearance",null,null,null,null,null,null,null,null,null,"mm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,"FPL",null,null,"flow pass length",null,null,null,null,null,null,null,null,null,"mm"]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WL1",null,"weir length",null,null,null,null,null,"mm"]
[]
[]
[]
[null,null,null,null,null,null,"２ pass tray の構造"]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A",null,"colume ID ",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B",null,"weir height",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H1",null,"downcomer width",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H3",null,"downcomer width",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D",null,"tray spacing",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E",null,"downcomer clearance",null,null,null,null,null,null,null,"mm"]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H1",null,"downcomer width",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H3",null,"downcomer width",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FPL",null,null,"flow pass length",null,null,null,null,null,null,"mm"]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WL1",null,"weir length",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"WL3",null,"weir length",null,null,null,null,null,null,null,"mm"]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,"４ pass tray の構造"]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"A",null,"colume ID ",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"B",null,"weir height",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"D",null,"tray spacing",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"E",null,"downcomer clearance",null,null,null,null,null,null,null,"mm"]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H1",null,"downcomer width",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H3",null,"downcomer width",null,null,null,null,null,null,null,"mm"]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"H5",null,"downcomer width",null,null,null,null,null,null,null,"mm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,null,"FPL",null,null,"flow pass length",null,null,null,null,null,null,"mm"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"液ロードが低い場合は、Tray上で液が均等に流れないので \"切り欠き\" を設置する場合がある。　これを Notched　Weir　と呼ぶ。"]
[null,null,null,"notched  weir"]

{"sheet":"精度","index":3,"n_rows":44,"n_cols":12,"rows_kept":44,"cut":false,"hidden":false,"merged":[]}
[null,null,"計算精度の表示"]
[null,null,"C-XXXX #1-2  A mode"]
[null,null,"Vapor Rate","(kg/h)",128874,128874]
[null,null,"Liquid Rate","(kg/h)",283056,283056]
[null,null,"Vapor Density","(kg/m3)",62.2,62.2]
[null,null,"Liquid Density","(kg/m3)",431.8,431.8]
[null,null,"Allowable Max.Flood%","(%)",82,82]
[null,"入","Foam factor","(-)",1,1]
[null,"力","Column ID","(mm)",3500,3500]
[null,"デ","Tray Spacing","(mm)",700,700]
[null,"｜","Tray thickness","(mm)",2,2]
[null,"タ","No of Flow Path(1 or 2 )","(-)",2,2]
[null,null,"h1","(mm)",647,647]
[null,null,"h3","(mm)",706,706,null,null,null,"A","B","C"]
[null,null,"h5","(mm)",0,0,null,"% FLOOD",null,70.900000000000006,70.798460185913655,{"$f":"K15/J15*100","v":99.856784465322491}]
[null,null,"Flow Pass Length","(mm)",750,750,null,"under downcomer velocity －１","(ft/s)",0.96,0.9650012496248721,100.52096350259086]
[null,null,"Weir Height","(mm)",40,40,null,"under downcomer velocity －２","(ft/s)",1.2010000000000001,1.2174263263758331,101.36772076401608]
[null,null,"Downcomer Clearance","(mm)",90.3,90.3,"計","pess.drop dry-1","inch liq",3.302,3.3260911644671545,100.72959310924151]
[null,null,"Downcomer Max.Backup","(%)",40,40,"算","pess.drop dry-1","inch liq",3.302,3.3260911644671545,100.72959310924151]
[null,null,"Downcomer Area Ratio","(-)",1,1,"結","pess.drop over weir-1","inch liq",2.2669999999999999,2.2668423486927125,99.993045817940569]
[null,null,"(bottom / top )",null,null,null,"果","pess.drop over weir-2","inch liq",1.9410000000000001,1.9415329941610837,100.02745977130776]
[null,null,"Valve Type (V1=1 , V4=2 )",null,"V1","V1",null,"pess.drop tray-1","mmH2O",{"$f":"5.001*13.6","v":68.013599999999997},68.250528750953734,100.34835496276295]
[null,null,"Valve Hole ID","(mm)",39,39,null,"pess.drop tray-2","mmH2O",{"$f":"4.738*13.6","v":64.436800000000005},64.682626837070103,100.38150069070795]
[null,null,"No of ValvePER TRAY","(-)",504,504,null,"DC backup -1","(%)",41,40.699035179059685,99.265939461121178]
[null,null,"Ratio of light type valve (%)","(-)",50,50,null,"DC backup -2","(%)",39.1,39.451001387736412,100.89770175891665]
[null,null,"Notched weir (yes=1 ,no=2)",null,"No","No",null,"unit referance","(%)",63.1,63.01795973997249,99.869983740051481]
[null,null,"Notch depth ","(mm)","****","****",null,"25% weep vapor load-1","(%)",8.5,4.392578125,51.677389705882348]
[null,null,"Notch pitch","(mm)","****","****",null,"25% weep vapor load-2","(%)",8.3000000000000007,"非収束","***"]
[]
[null,null,"C-XXXX #1-2  B mode",null,null,null,null,null,null,"A","B","C"]
[null,null,"Vapor Rate","(kg/h)",55499,{"$f":"E31","v":55499},null,"% FLOOD",null,31.6,31.558594156194332,{"$f":"K31/J31*100","v":99.868968848716236}]
[null,null,"Liquid Rate","(kg/h)",137569,{"$f":"E32","v":137569},null,"under downcomer velocity －１","(ft/s)",0.45500000000000002,0.45693978943343611,{"$f":"K32/J32*100","v":100.42632734800793}]
[null,null,"Vapor Density","(kg/m3)",62.63,{"$f":"E33","v":62.63},null,"under downcomer velocity －２","(ft/s)",0.59099999999999997,0.57646612316941903,97.540799182642829]
[null,null,"Liquid Density","(kg/m3)",443.2,{"$f":"E34","v":443.2},"計","pess.drop dry-1","inch liq",2.9870000000000001,2.947517878149946,98.678201478069838]
[null,null,null,null,null,null,"算","pess.drop dry-1","inch liq",2.9870000000000001,2.947517878149946,98.678201478069838]
[null,null,null,null,null,null,"結","pess.drop over weir-1","inch liq",1.377,1.3771314137947011,100.00954348545396]
[null,null,null,null,null,null,"果","pess.drop over weir-2","inch liq",1.179,1.1795024381470822,100.04261561892129]
[null,null,null,null,null,null,null,"pess.drop tray-1","mmH2O",56.24,55.77498798122263,99.173164973724454]
[null,null,null,null,null,null,null,"pess.drop tray-2","mmH2O",54.02,53.550223266244203,99.13036517261051]
[null,null,null,null,null,null,null,"DC backup -1","(%)",30.3,30.010690400101176,{"$f":"K40/J40*100","v":99.045182838617734}]
[null,null,null,null,null,null,null,"DC backup -2","(%)",29.8,29.801391894289246,{"$f":"K41/J41*100","v":100.00467078620552}]
[null,null,null,null,null,null,null,"unit referance","(%)",27.1,27.045074022410873,{"$f":"K42/J42*100","v":99.79732111590728}]
[null,null,null,null,null,null,null,"25% weep vapor load-1","(%)",19.3,21.953125,{"$f":"K43/J43*100","v":113.74676165803108}]
[null,null,null,null,null,null,null,"25% weep vapor load-2","(%)",19,20.392187499999999,{"$f":"K44/J44*100","v":107.32730263157895}]

{"sheet":"SIM","index":4,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":true,"merged":[]}

{"sheet":"記号表","index":5,"n_rows":41,"n_cols":6,"rows_kept":41,"cut":false,"hidden":false,"merged":[]}
["記号表"]
[null,"記号","内容","単位","マクロでの変数"]
[null,"AA","Active area","ｆｔ2","AAE"]
[null,"AAM","Minimum Active area","ｆｔ2"]
[null,"AD","Downcomer area","ｆｔ2","AD1E ,AD3E ,AD5E"]
[null,"ADM","Minimum Downcomer area","ｆｔ2","ADM"]
[null,"Ah","Hole area","ｆｔ2","HAA"]
[null,"AT","Column sectional area","ｆｔ2","ATE"]
[null,"ATM","Minimum Column sectional area","ｆｔ2"]
[null,"CAF","Capacity factor",null,"CAF"]
[null,"CAF0","Capacity factor uncorrected by system factor",null,"CAF0"]
[null,"CFS","Vapor rate","ft3/s","WFGF"]
[null,"DC","Downcomer clearance","inch","DCCL"]
[null,"DL","Liquid density","lb/ft3","DLE"]
[null,"Dv","Vapor density","lb/ft3","DGE"]
[null,"Dm","Valve Metal density","lb/ft3","DM"]
[null,"DT","Column diameter","ft","ID  (m)"]
[null,null,"System factor",null,"FF"]
[null,"FPL","flow path length","inch","FPLE"]
[null,"Fs","System factor",null,"FF"]
[null,"GPM","Liquid rate","gpm","WFLG"]
[null,"Hdc","Dowmcomer Backup","inch","HDCMA, HDCMB","偶数段、奇数段"]
[null,"HN","Depth of notch","inch"]
[null,"How","liquid height over weir ","inch","DP2A, DP2B","偶数段、奇数段"]
[null,"How'","liquid height over the bottom of a notch ","inch"]
[null,"Hud","Head loss under dowcomer","inch liquid","HUDA, HUDB","偶数段、奇数段"]
[null,"Hw","Outlet weir height","inch","HW"]
[null,"Hwi","Inlet weir height","inch"]
[null,"Li","length of inlet weir","inch","Wl1, WL3, WL5"]
[null,"Lwi","length of outlet weir","inch"]
[null,"NP","Number of liquid path",null,"NTPT"]
[null,"△P","Pressure drop through tray","inch liquid","DPTA, DPTB","偶数段、奇数段"]
[null,"△Pdry","Dry pressure drop through tray","inch liquid","PDRY"]
[null,"VDdsg","dowcomer design velocity","GPM/ft2","VDDSG"]
[null,"VDdsg*","VDdsg uncorrected by system factor","GPM/ft2"]
[null,"VDC","Downcomer volume","ft3/s"]
[null,"Vh","vapor velocity through holes","ft/s","VH"]
[null,"Vload","Design vapor load","ft3/s","VLOAD"]
[null,null,"CFS× （ Dv/(DL-Dv)）＾0.5"]
[null,"WN","Width of notch","inch"]
[null,"WFP","Average flow path width","inch"]

{"sheet":"test","index":6,"n_rows":46,"n_cols":17,"rows_kept":46,"cut":false,"hidden":true,"merged":[]}
[]
[null,1,128874,3.8416454982990116,3.5163361437673828,6.8482528935362427E-2,5.6120773463160543E-2,3046.1684146123507,2496.3057028523253,70764,2496.3057028523253,27.347489620018791,0.5,386622,128.874,386622,128.874]
[null,2,64501.436999999998,3.8416454982990116,3.5163361437673828,6.8482528935362427E-2,5.6120773463160543E-2,3046.1684146123507,2496.3057028523253,70764,2496.3057028523253,27.347489620018791,0.5,128874,64501.436999999998,128874,128.874]
[null,3,32315.155500000001,3.8416454982990116,3.5163361437673828,0.24351173749745497,0.21707911957020681,10831.635088304813,9655.8869508273401,70764,9655.8869508273401,6.3285862148517351,0.32273036949371886,64501.436999999998,32315.155500000001,64501.436999999998,128.874]
[null,4,16222.01475,3.8416454982990116,3.5163361437673828,0.67868079277070703,0.61384336416764018,30188.371058748442,27304.340194734024,70764,27304.340194734024,1.5916758835889286,0.1620087148954012,32315.155500000001,16222.01475,32315.155500000001,128.874]
[null,5,8175.444375,3.8416454982990116,3.5163361437673828,1.3678544316976868,1.2391945363987209,60843.473954616878,55120.55870338605,70764,55120.55870338605,0.28380411346688644,8.1647887596242419E-2,16222.01475,8175.444375,16222.01475,128.874]
[null,6,4152.1591875000004,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,8175.444375,4152.1591875000004,8175.444375,128.874]
[null,7,2140.5165937500001,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,4152.1591875000004,2140.5165937500001,4152.1591875000004,128.874]
[null,8,1134.6952968749999,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,2140.5165937500001,1134.6952968749999,2140.5165937500001,128.874]
[null,9,631.78464843749998,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,1134.6952968749999,631.78464843749998,1134.6952968749999,128.874]
[null,10,380.32932421875,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,631.78464843749998,380.32932421875,631.78464843749998,128.874]
[null,11,254.60166210937501,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,380.32932421875,254.60166210937501,380.32932421875,128.874]
[null,12,191.73783105468749,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,254.60166210937501,191.73783105468749,254.60166210937501,128.874]
[null,13,160.30591552734376,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,191.73783105468749,160.30591552734376,191.73783105468749,128.874]
[null,14,144.58995776367186,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,160.30591552734376,144.58995776367186,160.30591552734376,128.874]
[null,15,136.73197888183591,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,144.58995776367186,136.73197888183591,144.58995776367186,128.874]
[null,16,132.80298944091794,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,136.73197888183591,132.80298944091794,136.73197888183591,128.874]
[null,17,130.83849472045898,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,132.80298944091794,130.83849472045898,132.80298944091794,128.874]
[null,18,129.85624736022947,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,130.83849472045898,129.85624736022947,130.83849472045898,128.874]
[null,19,129.36512368011472,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,129.85624736022947,129.36512368011472,129.85624736022947,128.874]
[null,20,129.11956184005737,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,129.36512368011472,129.11956184005737,129.36512368011472,128.874]
[null,21,128.9967809200287,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,129.11956184005737,128.9967809200287,129.11956184005737,128.874]
[null,22,128.93539046001433,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.9967809200287,128.93539046001433,128.9967809200287,128.874]
[null,23,128.90469523000718,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.93539046001433,128.90469523000718,128.93539046001433,128.874]
[null,24,128.8893476150036,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.90469523000718,128.8893476150036,128.90469523000718,128.874]
[null,25,128.88167380750178,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.8893476150036,128.88167380750178,128.8893476150036,128.874]
[null,26,128.8778369037509,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.88167380750178,128.8778369037509,128.88167380750178,128.874]
[null,27,128.87591845187546,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.8778369037509,128.87591845187546,128.8778369037509,128.874]
[null,28,128.87495922593774,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87591845187546,128.87495922593774,128.87591845187546,128.874]
[null,29,128.87447961296886,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87495922593774,128.87447961296886,128.87495922593774,128.874]
[null,30,128.87423980648441,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87447961296886,128.87423980648441,128.87447961296886,128.874]
[null,31,128.87411990324222,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87423980648441,128.87411990324222,128.87423980648441,128.874]
[null,32,128.87405995162112,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87411990324222,128.87405995162112,128.87411990324222,128.874]
[null,33,128.87402997581057,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87405995162112,128.87402997581057,128.87405995162112,128.874]
[null,34,128.8740149879053,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87402997581057,128.8740149879053,128.87402997581057,128.874]
[null,35,128.87400749395266,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.8740149879053,128.87400749395266,128.8740149879053,128.874]
[null,36,128.87400374697631,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400749395266,128.87400374697631,128.87400749395266,128.874]
[null,37,128.87400187348817,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400374697631,128.87400187348817,128.87400374697631,128.874]
[null,38,128.8740009367441,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400187348817,128.8740009367441,128.87400187348817,128.874]
[null,39,128.87400046837206,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.8740009367441,128.87400046837206,128.8740009367441,128.874]
[null,40,128.87400023418604,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400046837206,128.87400023418604,128.87400046837206,128.874]
[null,41,128.87400011709303,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400023418604,128.87400011709303,128.87400023418604,128.874]
[null,42,128.87400005854653,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400011709303,128.87400005854653,128.87400011709303,128.874]
[null,43,128.87400002927325,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400005854653,128.87400002927325,128.87400005854653,128.874]
[null,44,128.87400001463664,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400002927325,128.87400001463664,128.87400002927325,128.874]
[null,45,128.87400000731833,3.8416454982990116,3.5163361437673828,1.6639898391835255,1.5078413490083438,74015.86023700943,67070.225983198587,70764,67070.225983198587,5.5073230522985288E-2,0.05,128.87400001463664,128.87400000731833,128.87400001463664,128.874]

{"sheet":"weep data","index":7,"n_rows":41,"n_cols":5,"rows_kept":41,"cut":false,"hidden":true,"merged":[]}
[null,null,2014.08,"Weeping 計算を下記データで計算するよう修正 "]
["weeping","Y","X","Z","Y"]
[null,"leak","head","Vload/AH","leak"]
["V-1","GPM","inch liq",null,"GPM"]
[null,0.28999999999999998,1,0.05,0.28999999999999998]
[null,0.79,2,0.05,0.79]
[null,1.27,3,0.05,1.27]
[null,1.73,4,0.05,1.73]
[null,0.12,1,0.15,0.12]
[null,0.34,2,0.15,0.34]
[null,0.55000000000000004,3,0.15,0.55000000000000004]
[null,0.76,4,0.15,0.76]
[null,0.03,1,0.25,0.03]
[null,0.14000000000000001,2,0.25,0.14000000000000001]
[null,0.23,3,0.25,0.23]
[null,0.33,4,0.25,0.33]
[null,-0.04,1,0.5,-0.04]
[null,0,2,0.5,0]
[null,3.5000000000000003E-2,3,0.5,3.5000000000000003E-2]
[null,7.4999999999999997E-2,4,0.5,7.4999999999999997E-2]
[]
[]
["weeping","Y","X","Z","Y"]
[null,"leak","head","Vload/AH","leak"]
["V-4","GPM","inch liq",null,"GPM"]
[null,0.18,1,0.1,{"$f":"B26","v":0.18}]
[null,0.64,2,0.1,{"$f":"B27","v":0.64}]
[null,1.1100000000000001,3,0.1,1.1100000000000001]
[null,1.59,4,0.1,1.59]
[null,0.11,1,0.3,0.11]
[null,0.38,2,0.3,0.38]
[null,0.67,3,0.3,0.67]
[null,0.96,4,0.3,0.96]
[null,0.06,1,0.4,0.06]
[null,0.26,2,0.4,0.26]
[null,0.47,3,0.4,0.47]
[null,0.68,4,0.4,0.68]
[null,0.02,1,0.6,0.02]
[null,0.15,2,0.6,0.15]
[null,0.27,3,0.6,0.27]
[null,0.39,4,0.6,0.39]

{"sheet":"%Flood詳細解説","index":8,"n_rows":40,"n_cols":6,"rows_kept":40,"cut":false,"hidden":false,"merged":[[42,1,42,3],[43,1,43,3],[44,1,44,3],[45,1,45,3],[36,1,36,3],[37,1,37,3],[38,1,38,3],[39,1,39,3],[40,1,40,3],[41,1,41,3]]}
[null,"％Floodの詳細解説"]
[]
[null,"％Flood は以下の式で計算される。 "]
[null,null,"Vload","Design vapor load","ft3/s","下記の計算式による"]
[null,null,"GPM","Liquid rate","gpm","液Load"]
[null,null,"FPL","flow path length","inch","シート”解説” の トレーの構造と名称 を参照"]
[null,null,"AA","Active area","ｆｔ2","シート”解説” の Active area を参照"]
[null,"CAFo はTS とVapor密度の関数で 下記のグラフを読み取る。マクロでは自動計算される","CAF0","Capacity factor uncorrected by system factor"]
[null,"TS: tray spacing が大きいと CAFo が大きくなるので ％Flood は小さくなる。",null,"System factor"]
[null,"（感覚的に理解できる 。）"]
[null,null,"Vload","Design vapor load","ft3/s"]
[null,null,null,"計算式：CFS× （ Dv/(DL-Dv)）＾0.5"]
[null,null,"CFS","Vapor rate","ft3/s"]
[null,null,"DL","Liquid density","lb/ft3"]
[null,null,"Dv","Vapor density","lb/ft3"]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[]
[null,"液Load （GPM） 、Vapor load （Vload) が大きくなれば %Flood は大きくなる。"]
[]
[null,"%FLOOD の定義は式（13） の通りである。 100%まで運転きるかというとそうではなく、GLITCH社は 式（13） の％FLOODを計算して、過圧（常圧を含む）の塔なら 通常の運転上限を82%、塔径が小さい場合や、バキューム塔の場合は 82%より小さい値を上限にする と定義している。 "]
[null,"全てのTray で 液、ガスの流量が脈動せず一定で、Foaming も起きないなら、 式(13)で 100% Flood まで 運転できるものと推測されるが、こんな運転はあり得ないし、ライセンサーも保証は出来ないので、設計点の液ガス 負荷 で 82% Flood を保障上限としているようである。\n設計点ベースの ２０%増しで 安定して運転したいのなら 、％Flood は 82/1.2＝68％ で 設計することになる。"]
[null,"%Flood 82 以上は、 上手く運転すれば運転できる可能性の領域であり、常時必ず運転できる範囲ではないので、テストランで短時間運転出来たからといって、常時其の運転を継続することには、危険が伴なうことを認識すべきである。"]
[null,"ADIP溶液の場合は system facotor ＝ 0.71 が指定されているので、同じ液、ガスロードでも、式(13)の %Flood は大きくなる。\n溶液ごとに 指定された system factor を用いて 式(13) の%Floodを計算して、運転の上限値は、 82％ と定義される。\nADIP溶液の場合  0.82*0.71 ＝0.58  なので ％Floodの 上限値は 58% という表現は 誤りである。"]

{"sheet":"Sheet1","index":9,"n_rows":0,"n_cols":0,"rows_kept":0,"cut":false,"hidden":false,"merged":[]}